Ref. 93142

.38-40 Winchester CF
        .38-40 Winchester CF M.1879
        .38 WCF
        .38 Winchester, Marlin & Colt
        .38 Winchester, Marlin & Remington
        .38-40 WCF
        .38-40 Winchester
        .38-40-160 Winchester

Diam. : 10,00            Length : 33,00            Cal : .38-40

ECRA	10033BBC010
EB	372
SAA	6545

Case	Bottlenecked
Bullet	Cylindro-ogival - flat tipped
Base	Rimmed
Priming	Boxer
Model	1880
Type	Standard
Use	Target practice
Country	USA
Manufact.	Union Metallic Cartridge Co. (UMC)
Factory	Bridgeport (Connecticut)
Headst.	U.M.C.  .38 C.L.M.R.

Bullet	Lead
Case	Brass
Mouth	Circle crimp
Primer	Copper
Powder	Smokeless

Bullet diam.	10,10	Mouth diam.	10,61	Neck diam.	10,61
Should. diam.	11,48	Head diam.	11,90	Rim diam.	13,09
Total length	40,14	Case length	33,09	Neck length	7,60
Should. length	22,00	Rim thickness	1,44	
Primer diam.	4,40
Cartr. weight : 20,000 g	Bullet weight : 11,660 g	

Notes	Fabrication antérieure à 1912, date à laquelle le sigle REM-UMC fut adopté.
La .38-40 est issue de la .44-40, introduite en 1874, avec un étui raccourci et rétreint à .38. Elle est apparue en 1880, destinée au Winchester Model 73 Lever-action. Colt a commencé peu après à chambrer des revolver avec ce calibre.